

1.修改link.lds



2.在board.c文件下增加代码



/\* Justin debug 添加一下代码，为了偏移开始地址\*/

**#define** RT\_APP\_PART\_ADDR 0x08020000

/\*\*

\* Justin debug

Function ota\_app\_vtor\_reconfig

Description Set Vector Table base location to the start addr of app(RT\_APP\_PART\_ADDR).

\*/

**static** **int** **ota\_app\_vtor\_reconfig**(**void**)

{

**#define** NVIC\_VTOR\_MASK 0x3FFFFF80

/\* Set the Vector Table base location by user application firmware definition \*/


SCB->VTOR = RT\_APP\_PART\_ADDR & NVIC\_VTOR\_MASK;

**return** 0;

}

INIT\_BOARD\_EXPORT(ota\_app\_vtor\_reconfig);

3.修改board.h



4.修改system\_stm32f4xx.c

